

一、创建项目文件



二、设置ui界面,设置页面



三、编写代码文件

MainWindow::**MainWindow**(QWidget \*parent) :

QMainWindow(parent),

ui(new Ui::MainWindow)

{

ui->setupUi(this);

COMPORT = new QSerialPort();

COMPORT->setPortName("COM4");

COMPORT->setBaudRate(QSerialPort::Baud9600);

COMPORT->setParity(QSerialPort::Parity::NoParity);

COMPORT->setDataBits(QSerialPort::DataBits::Data8);

COMPORT->setStopBits(QSerialPort::StopBits::OneStop);

COMPORT->setFlowControl(QSerialPort::FlowControl::NoFlowControl);

COMPORT->*open*(QIODevice::ReadWrite);

if(COMPORT->isOpen())

{

qDebug()<<"Serial Port is Connected.";

qDebug()<<COMPORT->error();

}

else

{

qDebug()<<"Serial Port is Not Connected.";

qDebug()<<COMPORT->error();

}

connect(COMPORT,SIGNAL(readyRead()),this,SLOT(Read\_Serial()));

}

MainWindow::~***MainWindow***()

{

delete ui;

}

void MainWindow::**on\_pushButton\_Send\_Data\_clicked**()

{

if(COMPORT->isOpen())

{

COMPORT->write(ui->lineEdit\_Send\_Data->text().toLatin1()+char(10));

COMPORT->flush();

qDebug()<<"Write Serial";

}

}

void MainWindow::**Read\_Serial**()

{

if(COMPORT->isOpen())

{

while(COMPORT->*bytesAvailable*())

{

Data\_From\_SerialPort += COMPORT->readAll();

}

if(Data\_From\_SerialPort.at(Data\_From\_SerialPort.length()-1)==char(10))

{

IS\_Data\_Received = true;

}

if(IS\_Data\_Received == true)

{

qDebug()<<"Data From Serial Port: "<<Data\_From\_SerialPort;

ui->textEdit->append(Data\_From\_SerialPort);

Data\_From\_SerialPort = "";

IS\_Data\_Received = false;

}

}

}

void MainWindow::**Read\_Data\_From\_Socket**()

{

if(TCPSocket)

{

if(TCPSocket->isOpen())

{

QByteArray Data\_From\_Server=TCPSocket->readAll();

QString MessageString = QString::fromStdString(Data\_From\_Server.toStdString());

ui->receive\_data\_box->append(MessageString);

}

}

}

四、运行结果

